Jakob Werle

Temple University | Fall 2023

Simulation Testing Methods for Improving Vehicle Dynamics

tECHNICAL cOMMUNICATION

**DRAFT**

**2024-11-11**

Abstract

# Executive Summary

Table of Contents

[Executive Summary 1](#_Toc182324513)

[Problem Analysis 4](#_Toc182324514)

[Overview of problem and its significance 4](#_Toc182324515)

[STEM fundamentals of problem 4](#_Toc182324516)

[Lessons from prior responses to the problem 5](#_Toc182324517)

[Project objectives and constraints 6](#_Toc182324518)

[Candidate Solutions 7](#_Toc182324519)

[Scope of solutions considered 7](#_Toc182324520)

[Track testing 7](#_Toc182324521)

[Vehicle simulation 8](#_Toc182324522)

[Shock dynamometer 8](#_Toc182324523)

[Shaker rig 8](#_Toc182324524)

[Kinematics and compliance testing 8](#_Toc182324525)

[Explanation of candidate solutions 8](#_Toc182324526)

[Candidate solution 1 8](#_Toc182324527)

[Candidate solution 2 8](#_Toc182324528)

[Candidate solution 3 8](#_Toc182324529)

[Comparative assessment of candidate solutions 8](#_Toc182324530)

[Project Recommendations 10](#_Toc182324531)

[Proposed solution 10](#_Toc182324532)

[Design and implementation challenges 10](#_Toc182324533)

[Anticipated project outcomes and impacts 10](#_Toc182324534)

[Glossary 11](#_Toc182324535)

[References 12](#_Toc182324536)

[Additional sources consulted 12](#_Toc182324537)

List of Figures

[Figure 1: Suspension System 5](#_Toc182324571)

[Figure 2: Ayrton Senna racing for McLaren 8](#_Toc182324572)

List of Tables

[Table 1: Potential Suspension Setup Options 7](#_Toc182324565)

[Table 2: Comparison of Candidate Solutions 8](#_Toc182324566)

# Problem Analysis

## Overview of problem and its significance

The basic goal of motorsport is for one driver and vehicle to negotiate a fixed distance faster than any other competitor (Smith, 1978). Drivers must manage varying track surface conditions, weather, traffic, the weight of fuel burning. Typically racing events are a combination of practice, qualifying, and racing sessions. The purpose of practice sessions is for drivers and teams to become acclimated with the new track and fine tune the vehicle’s setup package. Practice sessions are extremely valuable to racing teams as these are usually the only times that teams are willing to experiment. For series like Formula 1, teams are only granted two extra testing days throughout the entire season. Qualifying sessions see race cars outfitted in their fastest setup package, as their fastest lap time will designate in what place it will begin the race. Usually, race durations can vary from 15 minute sprints to 24 hour endurance formats. Either way, the race setup will be such that the vehicle is consistently drivable, has minimal tire wear, and is fuel efficient.

As testing time is limited, the methods used to dial in a vehicles’ setup has become increasingly important. Racecar Engineering magazine suggests that for teams to be competitive they have to take advantage of simulation tools. Improvements in technology have allowed the race car to be analyzed before it ever touches pavement. Suspension setup, in particular, is hypersensitive to specific drivers and tracks.

## STEM fundamentals of problem

The concept of tuning begins with the understanding that a race car is simply four tires and a driver outfitted with devices that allow it to negotiate a track as fast as possible. Changing the configuration of any devices in the correct way can aid the driver in driving the track faster and more efficiently. The most critical of the devices begins with tires. Tires receive all road inputs and generate all tractive forces, as they are the only parts of the car in contact with the road surface. There are two modes in which tires interact with the vehicle to produce traction – mechanically and aerodynamically. Mechanical grip is the result of the kinematic design of vehicle and setup of suspension components. Typical race cars have some form linkage that connects the wheels to the chassis. A spring and damper assembly allows the wheels to absorb bumps and just as importantly, control the motion of the chassis. Aerodynamic grip, which is produced by wings and bodywork, takes affect at higher speeds and is dependent on vehicle ride height and attitude.

Many of a vehicles dynamic parameters are designed directly into the chassis with regulations, packaging, and tire allocation in mind. This can make fundamental characteristics of a car challenging to adjust because large weldments and assemblies would need redesigned. Several parameters of racecar have been designed into a window of operation and have corresponding mechanical adjustments that can be made by a technician. The number and type of adjustments available varies with the type of car, typically with more complex systems found at higher levels of racing. Figure 1: Suspension System. Figure 1 displays a 3D rendering of the suspension linkages and wheel assemblies for the University of Padua’s Formula Student car.




Figure : Suspension System

What do dynamic tests yield for results? How are cars fine-tuned?

Gathering data for vehicle systems comes in a variety of methods but it always is focused on analyzing a particular metric. With that being said, most testing utilizes a variety of equipment. Most of the time the metric boils down to measuring a force, position, or acceleration of components. There are many ways to capture each vehicle parameter. For example, tire loads can be collected using load cells while driving or by monitoring feedback loop data from shaker rig posts.

Since one goal of improving suspension performance is minimizing wheel load divergence (insert citation), the data gathered needs to organized appropriately.

## Lessons from prior responses to the problem

Dynamic vehicle testing was first introduced to the laboratory environment in the 1950’s, with a focus on overall vehicle comfort and durability (Dodds & Plummer, 2001). Early testing apparatuses were designed using two-stage servo-valves and four linear actuators or posts, which were concurrently being developed by the Moog engineering company (Dodds & Plummer, 2001). To operate the testing rig, a vehicle was suspended in the air in which each post supported one of the vehicle’s wheels. The posts were actuated vertically in accordance to a testing cycle which aimed to statistically replicate a vehicle’s wheel travel (Dodds & Plummer, 2001). While subjective results reported good comfort, users noted potential error from the test setup lacking lateral and for/aft forces as well as inertial forces associated with rolling tires. Furthermore, some unresolved dynamics issue with hydraulics systems used throughout the 1960’s muddied the results from “excitement simulations” (Dodds & Plummer, 2001).

The next breakthrough in dynamic vehicle testing was “Response Simulation”. GM Truck and Bus conceived that by using a vehicle as the transducer, road inputs at the tire contact patch could be determined while driving at the proving grounds. The measured wheel response could then be used to drive closed loop control of the servo-hydraulic system (Dodds & Plummer, 2001). Implementing this system improved relevance of test results and lead to the creation of multiple testing software.

In order to increase accuracy of simulations, contemporary testing rigs have been configured to allow forces and motion in multiple directions. Triaxial systems have the ability to generate vertical, lateral, and longitudinal forces, and yaw and pitch moments at each wheel (Dodds & Plummer, 2001). These more complex setups allows analysis of vehicle characteristics such as self-aligning torque and braking, which would be possible on previous four-post rigs. However, the setup for these tests are significantly more complex and require an extra actuator for every degree of motion (Dodds & Plummer, 2001).

An alternative method called “Body Restraint Testing” applies force and moment inputs through the chassis rather than wheels. The significance of this technique is that the inputs can be relatively small and output displacements in vertical, pitch, and roll can be large (Dodds & Plummer, 2001). Initial passive restraint setups were disadvantaged by changing the structural loading of the chassis, which skewed results. To eliminate this issue, later setups replaced fixed chassis restraints with actuators which could apply high frequency motions but respond to low frequency loads (Dodds & Plummer, 2001). These systems proved to have versatile control of the vehicle’s body and could introduce external forces such as aerodynamics in motorsports.


A common configuration found today is called the “7-Post Rig”, in which four of the posts support the wheels and three posts support the chassis. The unique characteristic of this setup is that the wheels are supported by flat plates which allows road inputs to be generated without impeding the natural motion of the wheels. The remaining three posts, often referred to as “aeroloaders” can be used to generate aerodynamic forces seen above roughly 100mph (“Seven-Post Rigs,” n.d.). Unfortunately, aeroloaders have a tendency to dampen the vehicle’s natural response to road inputs by the wheel plates. To mitigate this, a compliant linkage can be arranged between the aeroloaders and chassis to allow loading with a sufficient amount of compliance to let the vehicle move unimpeded (“Seven-Post Rigs,” n.d.). This solution has it’s own issue, being that the added compliance does not allow the large downforce loads to be generated in the simulation. By using “velocity feed-forward” algorithms to predict the motion of the chassis in addition to a compliant link, a workable result emerges for downforce to be simulated on a seven post shaker rig (“Seven-Post Rigs,” n.d.).

## Project objectives and constraints

The goal of this project is to analyze existing forms of dynamic vehicle testing and suggest methods that will yield the most effective improvements to vehicle performance. It is explained that successful testing results are able to provide a variety of setup changes that would benefit the vehicle (“Seven-Post Rigs,” n.d.). Since racing events take place in ever changing conditions, being able to have options for vehicle behavior is beneficial. Good data is able to help an engineer draw correlations between parameters that might not have been seen without testing. Also it can narrow the window of what is understood to be suboptimal setup choices.

Another aspect of selecting a simulation method is determining the type and quantity of data points to be analyzed. Due to the decreasing costs of electronics and growth of technology, adding data acquisition to vehicles and testing apparatuses has become very accessible (Segers, 2014). Engineers can quickly add enough sensors to swamp the data logging system. In addition, the number of setup options can become overwhelming. As seen in Table 1: Potential Suspension Setup Options, for even a fairly standard vehicle package, the number of individual adjustments is significant.

Table : Potential Suspension Setup Options

It is desirable for the analysis to be efficient which requires the least amount of time between testing and results.

Ideally, using simulation testing tools decreases the cost for a racing team to be successful. Unfortunately, this reality is not feasible because the inevitable costs associated with more testing.

For a given series, the competitors will be made aware of what tracks they will race at far in advance. Since a unique setup is desirable for each track, simulation testing would be conducted for each racing event. A relationship can be made between the cost or quantity of testing conducted to the success per race of a team.

# Candidate Solutions

## Scope of solutions considered

### Track testing

The most basic form of tuning the race car is track side tuning. While track tuning does not take advantage of engineering tools and extra time found in a lab, it is worth understanding the most fundamental approach. Furthermore, for all methods that will be analyzed, track tuning will be remain as one the last steps in validating a setup adjustment.

A typical track tuning session consists of shaking down the car and running through a testing plan. The shake down is an essential step in which the car and driver are introduced to the new track. A testing plan is developed before the testing day and targets a particular segment of the vehicle. As progress is made with the vehicle’s performance, the testing plan can be adjusted to target more vital aspects of vehicle’s handling. Because adjustment decisions are made based on analyzing vehicle data and driver feedback after each session, the duration of the testing process can be lengthy.

Major benefits of track tuning are that the car will be in virtually the same environment as when it will compete. On a similar note, the vehicle’s components will respond to track stimuli in their natural way, which is something that is needs to be accounted for when putting the car on various testing rigs. The level at which testing is done comes down to the data acquisition system fitted to the vehicle and efficiency of the crew. A simple data system can cost hundreds to thousands of dollars. For lower levels of racing, the performance gain of a data system can be negligible without a track side engineer, which can significantly increase costs. Weather also needs to be factored in to a testing plan, as rain or accidents can have major effects on scheduling and performance results. Performance analysis is also limited to the vehicle’s data logging system, as the number and type of sensors used depends on the system’s available inputs. Custom logging systems allow full customization of data acquisition, but are typically found at higher levels of racing due to increased cost and development.

### Vehicle simulation

An alternative to testing the actual vehicle is using software to simulate performance.

### Shock dynamometer

### Shaker rig

### Kinematics and compliance testing

## Explanation of candidate solutions

### Candidate solution 1

### Candidate solution 2

### Candidate solution 3

A race car on a track

Description automatically generated

Figure 2: Ayrton Senna racing for McLaren

## Comparative assessment of candidate solutions

Blah blah blah

Table : Comparison of Candidate Solutions

|  |  |  |  |
| --- | --- | --- | --- |
| Criteria |  |  |  |
| Costs |  |  |  |
| Collection time |  |  |  |
| Processing time |  |  |  |
| Key data points |  |  |  |
| Setup requirements |  |  |  |
| Data vulnerability |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Project Recommendations

## Proposed solution

## Design and implementation challenges

## Anticipated project outcomes and impacts

# Glossary

# References

## Additional sources consulted

Dodds, C. J., & Plummer, A. R. (2001). *Laboratory Road Simulation for Full Vehicle Testing: A Review*. 2001-26–0047. https://doi.org/10.4271/2001-26-0047

Segers, J. (2014). *Analysis Techniques for Racecar Data Acquisition—Second Edition*. SAE International. https://doi.org/10.4271/R-408

Seven-post Rigs. (n.d.). *Racecar Engineering*.

Smith, C. (1978). *Tune to Win*.